<https://web.archive.org/web/20221209090535/https://www.photorobot.com/manuals/compatible-cameras>

# Compatible Cameras with PhotoRobot

*PhotoRobot supports a wide range of camera models.*

## Canon cameras

* EOS R /RP
* EOS R3 / R5 / R6 / R10
* EOS 5DS / EOS 5DS R
* EOS 40D / 50D / 60D / 70D / 77D / 80D / 90D
* EOS 1D Mark III / 1Ds Mark III / 1D Mark IV / 1D X / 1D C / 1D X Mark II / 5D Mark II / 5D Mark III / 5D Mark IV / 6D / 6D Mark II / 7D / 7D Mark II
* EOS 100D / 200D / 250D / 450D / 500D / 550D / 600D / 650D / 700D / 750D / 760D / 800D / 850D
* EOS DIGITAL / Kiss X2 / KISS F / Kiss X3 / Kiss X4 / Kiss X5 / Kiss X50 / Kiss X6i / Kiss X7i / Kiss X7 / Kiss X70 / Kiss X80 / Kiss X9i / Kiss X9 / Kiss M / Kiss X90
* EOS M / M2 / M3 / M5 / M6 / M10 / M50 / M100
* EOS 1000D / 1100D / 1200D / 1300D / 1500D / 2000D / 3000D / 4000D / 8000D / 9000D
* EOS DIGITAL REBEL XS / REBEL Xsi / REBEL T1i / REBEL T2i / REBEL T3i / REBEL T3 / REBEL T4i / REBEL T5i / REBEL SL1 / REBEL T5 / EOS REBEL T6s / REBEL T6i / Rebel T6 / Rebel T7i / Rebel SL2 / REBEL T7 / REBEL T100

Please note: Remote capture functions are not supported for the EOS M/EOS M2/EOS M3/EOS M10/EOS M5/EOS M6/EOS M100.

List of supported handheld [close-up and packshot cameras](https://web.archive.org/web/20221209090535/https://developers.canon-europe.com/developers/s/article/Latest-CCAPI).

## Nikon cameras

*Basic capture functions are supported for the following models (we recommend using Canon for full functions). For compatibility about specific Nikon models, please contact us.*

* Z7
* D810 / D850
* D7000

Disclaimer: There is limited support for Apple silicon (M1 and newer). The PhotoRobot Controls application needs to be run in Intel processor mode. Instructions can be found on the [Apple website](https://web.archive.org/web/20221209090535/https://support.apple.com/en-au/HT211861).

## 3rd party cameras

*We also support third party cameras under the following conditions. Please contact us for specific information.*

* The camera is fired with a cable trigger over PhotoRobot Control Unit.
* The transfer of photos from the camera is taken care of by 3rd-party SW installed on the PC. The SW transfers photos to the folder over which PhotoRobot Controls listen.

Please note: 3rd party cameras are supported from PhotoRobot Controls version 2.5.4

‌